
1    Printed Circuit Board (PCB)
1    2 x 13 pin Box Header
1    DB25-F Ribbon (ILDA Port)
1    1 x 6 Socket (signal inputs)
1    1 x 3 Socket (USB power input)
2    1 pin Socket (test points for V-off & GND)
4    2 pin Headers for Jumpers
4    Jumpers, red, green, blue, white
3    8 pin IC sockets
3    TLO72 op-amps
1    D106E DC/DC Converter
7    500 ohm 25 turn trim pots,  W501
6    100K ohm 25 turn trim pots, W104
6    10K 1% resistors, brown black black red brown
6    15K 1% resistors, brown green black red brown
1    120 ohm resistor, brown red black black brown
1    470 ohm resistor, yellow violet black black brown
4    5.1v zener diodes
5    10uF Tantalum Capacitors
1    LM337 Negative Voltage Regulator

It is critical to align all the parts in the proper orientation!
Note the location of the tops of the ICs and their sockets,
the polarity of the zener diodes and Tantalum capacitors.
Make sure the ribbon port header has the key slot toward the
inside of the PCB. All of these parts can easily be put in wrong
and that will not work!

The 470 ohm resistor goes in the place marked 500 on the PCB.
This resister is in series between the +5V USB power input
and pin 13, the shutter actuator, on the ILDA connector.

24AWG solid copper (telephone) wire fits nicely into the
inputs, USB voltage and test point sockets.

               ILDA PORT
            [:::::::::::::]
                  |-|  <- slot

 * GND          [  ^  ]  5v zener :
   (Off) (Gain) [TLO72] (Off) (Gain)
        X       [opamp]    Green

 * V_off        [  ^  ]  5v zener :
   (Off) (Gain) [TLO72] (Off) (Gain)
        Y       [opamp]     Blue

   : 5v zener   [  ^  ]  5v zener :
   (Off) (Gain) [TLO72] (Off) (Gain)
       Red      [opamp]   Intensity


   (adj)        [-vreg]
                        power
                        * * *
                      GND | GND
         INPUT           +5V
      * * * * * *
      X Y R G B I                   Extra Stimulus Inc. 2013


Go here!:
http://laserboy.org/forum/index.php?topic=561.0

